**Appendix A-2.2**

Proposed Regulation Order

Periodic Smoke Inspections of Heavy-Duty Diesel Powered Vehicles

[Note: This version of the Proposed Regulation Order is provided in a tracked changes format to improve the accessibility of the regulatory text. This version is not the authoritative version for this proposed rulemaking. The proposed amendments are incorporated into the current regulatory text for ease of readability only. For the authoritative version that complies with Government Code section 11346.2, subdivision (a)(3), please see Appendix A-2.1. To review this document in a clean format (no underline or strikeout to show changes), please [accept all tracked changes](https://support.microsoft.com/en-us/office/accept-or-reject-tracked-changes-in-word-b2dac7d8-f497-4e94-81bd-d64e62eee0e8).]

Chapter 3.6. Periodic Smoke Inspections of Heavy-Duty Diesel Powered Vehicles

Section 2193. Smoke Opacity Standards, Inspection Intervals, and Test Procedures (Proposed Amendments)

**Proposed Regulation Order**

Title 13, California Code of Regulations

Amend section 2193, title 13, California Code of Regulations, to read as follows:

(Note: Various portions of the regulation that are not modified by the proposed amendments are omitted from the text shown and indicated by “ \* \* \* \* \* ”.)

**2193. Smoke Opacity Standards, Inspection Intervals, and Test Procedures.**

(a) Standards. For any vehicle subject to the requirements of this chapter, the maximum smoke opacity standard when tested in accordance with the test procedures specified in section 2193(d) is as specified in section 2196.6.

\* \* \* \* \*

Note: Authority cited: Sections 39600, 39601, 43000.5, 43013 and 43701(a), Health and Safety Code. Reference: Sections 39002, 39003, 39033, 43000, 43013, 43018, 43701(a), and 44011.6, Health and Safety Code.