**Attachment A-2.2**

Final Regulation Order, Alternate/Accessible Format

Periodic Smoke Inspections of Heavy-Duty Diesel Powered Vehicles

[Note: This alternate version of the Final Regulation Order is provided in a tracked changes format to improve the accessibility of the regulatory text. This version is not the authoritative version for this rulemaking, nor is it additional regulatory text, but is an alternate/duplicate version provided for the purposes of improved accessibility. The amendments are incorporated into the current regulatory text for ease of readability only. For the authoritative version that complies with California Code of Regulations, title 1, section 8, subdivision (b), please see the pdf version titled, “Attachment A-2.1, Final Regulation Order.” To review this document in a clean format (no underline or strikeout to show changes), please select “Simple Markup” or “No Markup” in Microsoft Word’s Review menu. You can also change the view to the original (current regulatory text prior to proposed amendments) by selecting “Original. Additionally, “Advanced Track Changes Options” will allow for further options regarding color and other markings. Instructions on using/viewing Track Changes can be found [here](https://support.microsoft.com/en-us/office/track-changes-in-word-197ba630-0f5f-4a8e-9a77-3712475e806a)]

Chapter 3.6. Periodic Smoke Inspections of Heavy-Duty Diesel Powered Vehicles

Section 2193. Smoke Opacity Standards, Inspection Intervals, and Test Procedures (Proposed Amendments)

**Final Regulation Order**

Title 13, California Code of Regulations

Amend section 2193, title 13, California Code of Regulations, to read as follows:

(Note: The amendments to existing regulatory language are shown in ~~strikethrough~~ to indicate deletions and underline to indicate additions. Various portions of the regulation that are not modified by the proposed amendments are omitted from the text shown and indicated by “ \* \* \* \* \* ”.)

**2193. Smoke Opacity Standards, Inspection Intervals, and Test Procedures.**

(a) Standards. For any vehicle subject to the requirements of this chapter, the maximum smoke opacity standard when tested in accordance with the test procedures specified in section 2193(d) is as specified in section 2196.6.

\* \* \* \* \*

Note: Authority cited: Sections 39600, 39601, 43000.5, 43013 and 43701(a), Health and Safety Code. Reference: Sections 39002, 39003, 39033, 43000, 43013, 43018, 43701(a), and 44011.6, Health and Safety Code.